PANELIZED: Not panelized

MATERIAL: FPC flexible board

LAYERS: 2

FINISHED BOARD THICKNESS: 0.2mm

PAD TREATMENT: Immersion gold

OUTER COPPER THICKNESS: 1 oz

IMMERSION GOLD THICKNESS: 1μ

COVERLAY COLOR: Yellow

COVERLAY THICKNESS: 25μm

LEGEND: White

REINFORCEMENT METHOD: PI reinforcement (See TOP PASTER for reinforcement areas)

REINFORCEMENT THICKNESS: 0.15mm